**AX181103 CRUISE REPORT**

During the first hours of NOV 20 wind increased considerably reaching gale force with steady winds of 45 knots. XBT cables started to tangle with each other giving questionable records at the end of the run. Unfortunately weather conditions made it unadvisable to work on deck at that time. Starting the run from the 200m isobath required 60 probes for the first HD part instead of 40**.**