File format of SFMR .dat files

Columns from left to right are:

Date of SFMR observation (YYYYMMDD)
Time (UTC) of SFMR observation (HHMMSS)
Longitude of SFMR observation (deg E)
Latitude of SFMR observation (deg N)
Radar Altitude (m)
Roll angle (deg)
Pitch angle (deg)
Air Temperature (C)
Sea Surface Temperature (C)
Salinity (g/kg)
SFMR Wind Speed (m/s)
SFMR Rain Rate (mm/hr)
Flight level wind speed (m/s)
Flight level wind direction (deg. meteorological)
Validity Flag (0=valid data, 1=questionable data, 2=invalid data, 3=no solution)
SFMR unit serial number
Number of good channels
Channel 1 (4.74 GHz) Brightness Temperature (K)
Channel 2 (5.31 GHz) Brightness Temperature (K)
Channel 3 (5.57 GHz) Brightness Temperature (K)
Channel 4 (6.02 GHz) Brightness Temperature (K)
Channel 5 (6.69 GHz) Brightness Temperature (K)
Channel 6 (7.09 GHz) Brightness Temperature (K)