**Cruise Report: AX8 Mar 2007**

a) XBT’s deployed: 239

b) Problem: The first couple of meters (0-3) gives a flat line, and it is not consistent. There were some bad drops when the wind picked up on the afternoon of the 20th.

c) Recommendations:

d) Other narrative:

e) Drifters deployed: See log sheet

f) ARGO floats deployed: NONE

**NOAA/AOML/PHOD DRIFTER LOG SHEET**

Cruise: AX80307

Technician: Pieter Truter

Ship: Safmarine Gonubie

Call Sign: DGVB

|  |  |  |  |
| --- | --- | --- | --- |
| **Number** | **S/N** | **Deploy Date/**  **Time**  **MMDDYYYY HHMM** | **Lat/Long**  **Deg Min X Deg Min X** |
| 1 | 62246 | 03/04/2007 20:07 | 15º 00.000' S 006º 06.870' W |
| 2 | 62247 | 03/06/2007 19:28 | 05º 00.001' S 016º 16.652' W |
| 3 | 62248 | 03/14/2007 01:16 | 04º 59.998' N 026º 30.308' W |
| 4 | 62245 | 03/15/2007 02:53 | 09º 59.998' N 032º 22.556' W |